I submit that allocation of frequencies in the 60m band would allow more continuity in communications between Amateur radio stations bridging a gap in propagation between the 80m and 40m bands.